
**CN LAB-08a (18/08/2023)**


**USN: 1BM21CS172**


**Create a topology in order to depict TTL of a packet.**


TOPOLOGY:



ROUTER CONFIG:











SENDING THE PDU NOTING THE DROP OF TTL VALUE AS IT CROSSES A ROUTER


PC-0 -> PC-1











PC-1 ->PC-0

